
-----------------------------------
       Cantera C++ examples
-----------------------------------




>>>>>  example 1

Description:
Ignition simulation using class IdealGasPhase with file gri30.yaml.
Constant-pressure ignition of a hydrogen/oxygen/nitrogen mixture
beginning at T = 1001 K and P = 1 atm.
 Tfinal = 2663.78
Output files:
  kin1.csv    (Excel CSV file)
  kin1.dat    (Tecplot data file)




>>>>>  example 2

Description:
Ignition simulation using class IdealGasPhase with file gri30.yaml.
Constant-pressure ignition of a hydrogen/oxygen/nitrogen mixture
beginning at T = 1001 K and P = 1 atm.
 Tfinal = 2663.78
Output files:
  kin3.csv    (Excel CSV file)
  kin3.dat    (Tecplot data file)




>>>>>  example 3

Description:
Chemical equilibrium.
Equilibrium composition and pressure for a range of temperatures at constant density.

CanteraWarning: NasaPoly2::validate:
For species SI2H6, discontinuity in h/RT detected at Tmid = 1000
        Value computed using low-temperature polynomial:  19.8328
        Value computed using high-temperature polynomial: 19.9055

CanteraWarning: NasaPoly2::validate:
For species SI2H6, discontinuity in s/R detected at Tmid = 1000
        Value computed using low-temperature polynomial:  49.5493
        Value computed using high-temperature polynomial: 49.7214

CanteraWarning: NasaPoly2::validate:
For species SI3H8, discontinuity in h/RT detected at Tmid = 1000
        Value computed using low-temperature polynomial:  29.3028
        Value computed using high-temperature polynomial: 29.4297

CanteraWarning: NasaPoly2::validate:
For species SI3H8, discontinuity in s/R detected at Tmid = 1000
        Value computed using low-temperature polynomial:  65.9731
        Value computed using high-temperature polynomial: 66.2781

CanteraWarning: NasaPoly2::validate:
For species SI2, discontinuity in h/RT detected at Tmid = 1000
        Value computed using low-temperature polynomial:  74.0115
        Value computed using high-temperature polynomial: 74.0387

CanteraWarning: NasaPoly2::validate:
For species SI2, discontinuity in s/R detected at Tmid = 1000
        Value computed using low-temperature polynomial:  32.8813
        Value computed using high-temperature polynomial: 32.9489

Output files:
  eq1.csv    (Excel CSV file)
  eq1.dat    (Tecplot data file)




>>>>>  example 4

Description:
Mixture-averaged transport properties.
Viscosity, thermal conductivity, and mixture-averaged
diffusion coefficients at 2 atm for a range of temperatures
Output files:
  tr1.csv    (Excel CSV file)
  tr1.dat    (Tecplot data file)




>>>>>  example 5

Description:
Multicomponent transport properties.
Viscosity, thermal conductivity, and thermal diffusion
 coefficients at 2 atm for a range of temperatures
Output files:
  tr2.csv    (Excel CSV file)
  tr2.dat    (Tecplot data file)
