type 2
version_major 0
version_minor 0
node_from 0
node_to 1
weight 20
min_latency 0
max_latency 0
min_bandwidth 0
max_bandwidth 32000
recommended_transfer_size 0
recommended_sdma_engine_id_mask 1
flags 3
