-- This reservoir simulation deck is made available under the Open Database
-- License: http://opendatacommons.org/licenses/odbl/1.0/. Any rights in
-- individual contents of the database are licensed under the Database Contents
-- License: http://opendatacommons.org/licenses/dbcl/1.0/

-- Copyright (C) 2015 Statoil

-- Norne full field model for SPE ATW 2013
RUNSPEC

DIMENS
46 112 22   /

--NOSIM

GRIDOPTS
 'YES' 0 /

OIL

WATER

GAS

DISGAS

VAPOIL

ENDSCALE
NODIR   REVERS /

METRIC

SATOPTS
HYSTER  /

START
 06  'NOV' 1997 /

EQLDIMS
 5  100  20 /

EQLOPTS
 'THPRES'  /   no fine equilibration if swatinit is being used

REGDIMS
-- ntfip  nmfipr  nrfreg  ntfreg
    22      3      1*      20    /

TRACERS
--  oil  water  gas  env
    1*   7      1*    1*   /
 
WELLDIMS
 130  36  15  84 /

TABDIMS
--ntsfun ntpvt nssfun nppvt ntfip nrpvt ntendp
   2     2     33     60   16    60 /

-- WI_VFP_TABLES_080905.INC = 10-20
VFPIDIMS
 30    20   20 /

-- Table no.
-- DevNew.VFP        = 1
-- E1h.VFP           = 2
-- AlmostVertNew.VFP = 3
-- GasProd.VFP       = 4
-- NEW_D2_GAS_0.00003.VFP = 5
-- GAS_PD2.VFP = 6
-- pd2.VFP           = 8 (flowline south)
-- pe2.VFP           = 9 (flowline north)
-- PB1.PIPE.Ecl  = 31
-- PB2.PIPE.Ecl  = 32  
-- PD1.PIPE.Ecl  = 33  
-- PD2.PIPE.Ecl  = 34 
-- PE1.PIPE.Ecl  = 35
-- PE2.PIPE.Ecl  = 36
-- B1BH.Ecl = 37
-- B2H.Ecl  = 38
-- B3H.Ecl  = 39
-- B4DH. Ecl= 40
-- D1CH.Ecl = 41
-- D2H.Ecl  = 42
-- D3BH.Ecl = 43

-- E1H.Ecl  = 45 
-- E3CH.Ecl = 47
-- K3H.Ecl  = 48


VFPPDIMS
 19  10  10  10  0  50 /

FAULTDIM
10000 /

PIMTDIMS
1  51 /

NSTACK
 30 /

UNIFIN
UNIFOUT

--FMTOUT
--FMTIN

OPTIONS
77* 1 /

---------------------------------------------------------
--
--	Input of grid geometry
--
---------------------------------------------------------
GRID

NEWTRAN

-- Ask for an EGRID file; no .GRID output.
GRIDFILE
  0  1 /

-- optional for postprocessing of GRID
MAPAXES
 0.  100.  0.  0.  100.  0.  /

GRIDUNIT
METRES  /

-- requests output of INIT file
INIT

MESSAGES
 8*10000  20000 10000 1000 1* /

PINCH
 0.001 GAP  1* TOPBOT TOP/

NOECHO

--------------------------------------------------------
--
--  	Grid and faults
--
--------------------------------------------------------

-- Simulation grid, with slooping faults:
-- file in UTM coordinate system, for importing to DecisionSpace
INCLUDE
 './INCLUDE/GRID/IRAP_1005.GRDECL' / 

--
INCLUDE
 './INCLUDE/GRID/ACTNUM_0704.prop' / 

-- Faults
INCLUDE
 './INCLUDE/FAULT/FAULT_JUN_05.INC' / 

-- Alteration of transmiscibility by use of the 'MULTFLT' keyword
INCLUDE
 './INCLUDE/FAULT/FAULTMULT_AUG-2006.INC' / 

--------------------------------------------------------
--
--  	Input of grid parametres
--
--------------------------------------------------------

--
INCLUDE
 './INCLUDE/PETRO/PORO_0704.prop' / 

INCLUDE
 './INCLUDE/PETRO/NTG_0704.prop' / 

INCLUDE
 './INCLUDE/PETRO/PERM_0704.prop' / 

COPY
   PERMX PERMY /
   PERMX PERMZ /
/

-- based on same kv/kh factor
MULTIPLY
   'PERMZ' 0.2    1 46 1 112  1  1 /    Garn 3
   'PERMZ' 0.04   1 46 1 112  2  2 /    Garn 2
   'PERMZ' 0.25   1 46 1 112  3  3 /    Garn 1
   'PERMZ' 0.0    1 46 1 112  4  4 /    Not 	(inactive anyway)
   'PERMZ' 0.13   1 46 1 112  5  5 /    Ile 2.2
   'PERMZ' 0.13   1 46 1 112  6  6 /    Ile 2.1.3
   'PERMZ' 0.13   1 46 1 112  7  7 /    Ile 2.1.2
   'PERMZ' 0.13   1 46 1 112  8  8 /    Ile 2.1.1
   'PERMZ' 0.09   1 46 1 112  9  9 /    Ile 1.3
   'PERMZ' 0.07   1 46 1 112 10 10 /    Ile 1.2
   'PERMZ' 0.19   1 46 1 112 11 11 /    Ile 1.1
   'PERMZ' 0.13   1 46 1 112 12 12 /    Tofte 2.2
   'PERMZ' 0.64   1 46 1 112 13 13 /	Tofte 2.1.3
   'PERMZ' 0.64   1 46 1 112 14 14 /	Tofte 2.1.2
   'PERMZ' 0.64   1 46 1 112 15 15 /	Tofte 2.1.1
   'PERMZ' 0.64   1 46 1 112 16 16 /	Tofte 1.2.2
   'PERMZ' 0.64   1 46 1 112 17 17 /	Tofte 1.2.1
   'PERMZ' 0.016  1 46 1 112 18 18 /	Tofte 1.1
   'PERMZ' 0.004  1 46 1 112 19 19 /	Tilje 4
   'PERMZ' 0.004  1 46 1 112 20 20 /	Tilje 3
   'PERMZ' 1.0    1 46 1 112 21 21 /	Tilje 2
   'PERMZ' 1.0    1 46 1 112 22 22 /	Tilje 1
/


--------------------------------------------------------
--
--      Barriers
--
--------------------------------------------------------

-- MULTZ multiplies the transmissibility between blocks
-- (I, J, K) and (I, J, K+1), thus the barriers are at the
-- bottom of the given layer.

-- Region barriers
INCLUDE
 './INCLUDE/PETRO/MULTZ_HM_1.INC' / 

-- Field-wide barriers
EQUALS
  'MULTZ'    1.0      1  46  1 112   1   1  / Garn3       - Garn 2
  'MULTZ'    0.05     1  46  1 112  15  15  / Tofte 2.1.1 - Tofte 1.2.2
  'MULTZ'    0.001    1  46  1 112  18  18  / Tofte 1.1   - Tilje 4
  'MULTZ'    0.00001  1  46  1 112  20  20  / Tilje 3     - Tilje 2
-- The Top Tilje 2 barrier is included as MULTREGT = 0.0
/

-- Local barriers
INCLUDE
 './INCLUDE/PETRO/MULTZ_JUN_05_MOD.INC' / 
  
  
-- 20 flux regions generated by the script Xfluxnum
INCLUDE
 './INCLUDE/PETRO/FLUXNUM_0704.prop' / 

-- modify transmissibilites between fluxnum using MULTREGT
INCLUDE
 './INCLUDE/PETRO/MULTREGT_D_27.prop' / 

NOECHO

MINPV
  500 /

EDIT
--------------------------------------------------------------------------------

--------------------------------------------------------------------------------
  
PROPS
--------------------------------------------------------------------------------
--
--    Input of fluid properties and relative permeability
--
---------------------------------------------------------

NOECHO

INCLUDE
'./INCLUDE/PVT/PVT-WET-GAS.INC' / 

TRACER
SEA  WAT  /
HTO  WAT  /
S36  WAT  /
2FB  WAT  /
4FB  WAT  /
DFB  WAT  /
TFB  WAT  /
/

-- initial water saturation
INCLUDE
'./INCLUDE/PETRO/SWINITIAL.INC' /

-- relative perm.
INCLUDE
'./INCLUDE/RELPERM/SCAL_NORNE.INC' /

SCALECRS
YES /

-- endpoints may be used as tuning papameters
EQUALS
SWL 0.04 1 46 1 112 1  1   / 
SWL 0.05 1 46 1 112 2  2   / 
SWL 0.15 1 46 1 112 3  3   / 
SWL 0.15 1 46 1 112 4  4   / 
SWL 0.05 1 46 1 112 5  10  / Ile 2.2.2 and Ile 2.2.1, Ile 2.1.3, Ile 2.1.2, and Ile 2.1.1 Ile 1.3 and Ile 1.2
SWL 0.16 1 46 1 112 11 12  / ile 1.1 and tofte 2.2
SWL 0.07 1 46 1 112 13 15  / tofte 2.1
SWL 0.06 1 46 1 112 16 16  / tofte 1.2.2
SWL 0.12 1 46 1 112 17 22  / Tofte 1.2.1, Tofte 1.2.1, tofte 1.1, tilje 
/

COPY
  SWL SWCR /
  SWL SGU  /
/


ADD
SWCR   0.08  1 46 1 112 1 22  /
/

-- SGU = 1 - SWL
MULTIPLY
SGU  -1  1 46 1 112 1 22  /
/

ADD
SGU   1  1 46 1 112 1 22  /
/

EQUALS
SGL   0.0  1 46 1 112 1 22  /
SGCR  0.03 1 46 1 112 1 22  /
SOWCR 0.13 1 46 1 112 1 22  /
SOGCR 0.07 1 46 1 112 1 22  /
SWU   1.0  1 46 1 112 1 22  /
/

-- Hysteresis input
EHYSTR
   0.1   0  0.1 1* KR /

COPY
 'SWCR'  'ISWCR'   1 46 1 112  5  22 /
 'SGU'   'ISGU'    1 46 1 112  5  22 /
 'SWL'   'ISWL'    1 46 1 112  5  22 /
 'SWU'   'ISWU'    1 46 1 112  5  22 /
 'SGL'   'ISGL'    1 46 1 112  5  22 /
 'SOGCR' 'ISOGCR'  1 46 1 112  5  22 /
 'SOWCR' 'ISOWCR'  1 46 1 112  5  22 /
 /

EQUALS
ISGCR 0.22 1 46 1 112  1  22 /
/

RPTPROPS
1 1 1 5*0 0 /
--------------------------------------------------------------------------------


REGIONS

--
INCLUDE
'./INCLUDE/PETRO/FIPNUM_0704.prop' / 

EQUALS
'SATNUM'  1    1  46  1   112    1  22  / 
'IMBNUM'  2    1  46  1   112    1  22  /
'PVTNUM'  1    1  46  1   112    1  22  /
/

INCLUDE
 './INCLUDE/PETRO/EQLNUM_0704.prop' / 

-- extra regions for geological formations and numerical layers 
--INCLUDE
-- './INCLUDE/PETRO/EXTRA_REG.inc' / 

---------------------------------------------------------------------------------

SOLUTION

RPTRST
BASIC=2 KRO KRW KRG /

RPTSOL

FIP=3  SWAT / 

---------------------------------------------------------------------------------
-- equilibrium data: do not include this file in case of RESTART

INCLUDE
'./INCLUDE/PETRO/E3.prop' / 

THPRES
  1 2 0.588031 /
  2 1 0.588031 /
  1 3 0.787619 /
  3 1 0.787619 /
  1 4 7.00083  /
  4 1 7.00083  /
/

-- initialise injected tracers to zero
TVDPFSEA
1000   0.0
5000   0.0 /
TVDPFHTO
1000   0.0
5000   0.0 /
TVDPFS36
1000   0.0
5000   0.0 /
TVDPF2FB
1000   0.0
5000   0.0 /
TVDPF4FB
1000   0.0
5000   0.0 /
TVDPFDFB
1000   0.0
5000   0.0 /
TVDPFTFB
1000   0.0
5000   0.0 /

-------------------------------------------------------------------------------

SUMMARY

NEWTON
MLINEARS

--
INCLUDE
 './INCLUDE/SUMMARY/summary.data' / 

--
--INCLUDE
-- './INCLUDE/SUMMARY/extra.inc' /

--
INCLUDE
 './INCLUDE/SUMMARY/tracer.data' / 
--
INCLUDE
 './INCLUDE/SUMMARY/gas.inc' / 

--
INCLUDE
 './INCLUDE/SUMMARY/wpave.inc' / 

--------------------------------------------------------------------------------


SCHEDULE


DRSDT
 0  /

NOECHO

--------------------------------------------
--=======Production Wells========--
-------------------------------------------- 

--
INCLUDE
 './INCLUDE/VFP/DevNew.VFP' / 

--
INCLUDE
 './INCLUDE/VFP/E1h.VFP' / 
--
INCLUDE
 './INCLUDE/VFP/NEW_D2_GAS_0.00003.VFP' / 
--
INCLUDE
 './INCLUDE/VFP/GAS_PD2.VFP' / 
--
INCLUDE
 './INCLUDE/VFP/AlmostVertNew.VFP' / 
--
INCLUDE
 './INCLUDE/VFP/GasProd.VFP' / 
  
 
-- 01.01.07 new VFP curves for producing wells, matched with the latest well tests in Prosper. lmarr

--
INCLUDE
 './INCLUDE/VFP/B1BH.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/B2H.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/B3H.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/B4DH.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/D1CH.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/D2H.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/D3BH.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/E1H.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/E3CH.Ecl' / 
--
INCLUDE
 './INCLUDE/VFP/K3H.Ecl' / 
 
--------------------------------------------
--=======Production Flowlines========--
-------------------------------------------- 
--
-- 16.5.02 new VFP curves for southgoing PD1,PD2,PB1,PB2 flowlines -> pd2.VFP
--
INCLUDE
 './INCLUDE/VFP/pd2.VFP' / 
--
-- 16.5.02 new VFP curves for northgoing PE1,PE2 flowlines -> pe2.VFP
--
INCLUDE
 './INCLUDE/VFP/pe2.VFP' / 
 
  
-- 24.11.06 new matched VLP curves for PB1 valid from 01.07.06
--
INCLUDE
 './INCLUDE/VFP/PB1.PIPE.Ecl' / 

--24.11.06 new matched VLP curves for PB2 valid from 01.07.06
--
INCLUDE
 './INCLUDE/VFP/PB2.PIPE.Ecl' / 

--24.11.06 new matched VLP curves for PD1 valid from 01.07.06
--
INCLUDE
 './INCLUDE/VFP/PD1.PIPE.Ecl' / 

--24.11.06 new matched VLP curves for PD2 valid from 01.07.06
--
INCLUDE
 './INCLUDE/VFP/PD2.PIPE.Ecl' / 

--24.11.06 new matched VLP curves for PE1 valid from 01.07.06
--
INCLUDE
 './INCLUDE/VFP/PE1.PIPE.Ecl' / 

--24.11.06 new matched VLP curves for PE2 valid from 01.07.06
--
INCLUDE
 './INCLUDE/VFP/PE2.PIPE.Ecl' / 
  
   
-------------------------------------------
--=======INJECTION FLOWLINES 08.09.2005     ========--
--------------------------------------------
-- VFPINJ nr. 10 Water injection flowline WIC 
--
INCLUDE
 './INCLUDE/VFP/WIC.PIPE.Ecl' / 

-- VFPINJ nr. 11 Water injection flowline WIF 
--
INCLUDE
 './INCLUDE/VFP/WIF.PIPE.Ecl' / 

--------------------------------------------
--=======   INJECTION Wells 08.09.2005       ========--
--------------------------------------------
-- VFPINJ nr. 12 Water injection wellbore Norne C-1H 
--
INCLUDE
 './INCLUDE/VFP/C1H.Ecl' / 

-- VFPINJ nr. 13 Water injection wellbore Norne C-2H 
--
INCLUDE
 './INCLUDE/VFP/C2H.Ecl' / 

-- VFPINJ nr. 14 Water injection wellbore Norne C-3H 
--
INCLUDE
 './INCLUDE/VFP/C3H.Ecl' / 

-- VFPINJ nr. 15 Water injection wellbore Norne C-4H 
--
INCLUDE
 './INCLUDE/VFP/C4H.Ecl' / 

-- VFPINJ nr. 16 Water injection wellbore Norne C-4AH 
--
INCLUDE
 './INCLUDE/VFP/C4AH.Ecl' / 

-- VFPINJ nr. 17 Water injection wellbore Norne F-1H 
--
INCLUDE
 './INCLUDE/VFP/F1H.Ecl' / 

-- VFPINJ nr. 18 Water injection wellbore Norne F-2H 
--
INCLUDE
 './INCLUDE/VFP/F2H.Ecl' / 

-- VFPINJ nr. 19 Water injection wellbore Norne F-3 H
--
INCLUDE
'./INCLUDE/VFP/F3H.Ecl' / 

-- VFPINJ nr. 20 Water injection wellbore Norne F-4H 
--
INCLUDE
'./INCLUDE/VFP/F4H.Ecl' / 

TUNING
1 10  0.1  0.15  3  0.3  0.3  1.20  /
5*   0.1   0.0001   0.02  0.02  /
2* 40 1* 15 /
/

-- only possible for ECL 2006.2+ version
ZIPPY2
'SIM=4.2' 'MINSTEP=1E-6' /

-- PI reduction in case of water cut
INCLUDE
'./INCLUDE/PI/pimultab_low-high_aug-2006.inc' / 

-- History
INCLUDE
'./INCLUDE/BC0407_HIST01122006.SCH' / 

END
