-- Synthetic test deck based on Norne. This data set is meant to be a simple,
-- well-documented deck for the behaviour of SUMMARY specified output. Data
-- is mostly entered to *traceable* and does not necessarily make sense from
-- a simulation point of view.

START
10 MAI 2007 /
RUNSPEC

TITLE
SUMMARYTESTS

-- A simple 10x10x10 cube. Simple to reason about, large enough for all tests
DIMENS
 10 10 10 /

REGDIMS
  10 /

OIL
GAS
WATER

UNIFIN
UNIFOUT

GRID

DX
1000*1 /
DY
1000*1 /
DZ
1000*1 /
TOPS
100*1 /

-- Cell 2,1,10 is inactive
ACTNUM
  901*1 0 98*1 /
  
PORO
1000*0.2 /

PERMX
  1000*0.25/

COPY
  PERMX PERMY /
  PERMX PERMZ /
/


REGIONS

FIPNUM
   100*1
   100*2
   100*3
   100*4
   100*5
   100*6
   100*7
   100*8
   100*9
   100*10 /
   

SUMMARY
DATE
PERFORMA
--
-- Field Data
-- Production Rates
FVPR
FWPR
FWPRH
FOPR
FOPRH
FGPR
FGPRH
FLPR
FLPRH
FGSR
FGCR
FNPR -- solvent
FCPR
--FTPRSEA
-- Injection Rates
FVIR
FWIR
FWIRH
FGIR
FNIR -- solvent
FGIRH
-- Production Cummulatives
FVPT
FWPT
FOPT
FLPT
FLPTH
FGPT
FNPT
FOPTH
FGPTH
FWPTH
FGST
FGCT
FCPT
-- Injection Cummulatives
FVIT
FWIT
FWITH
FGIT
FNIT
FGITH
-- In place
FWIP
FOIP
FGIP
-- Ratios
FWCT
FWCTH
FGOR
FGORH

-- From model2
FMWPR
FMWIN
FOE

-- Pressures
FPR

BPR
  1  1  1 /
  1  1  2 /
  1  1  3 /
  1  1  4 /
  1  1  5 /
  1  1  6 /
  1  1  7 /
  1  1  8 /
  1  1  9 /
  1  1  10 /    
  2  1  10 /  -- This cell is not ACTIVE
/

BSGAS
  1  1  1 /
/


BSWAT
  1  1  1 /
/


--  Region data
RPR
/
ROPT
/
RGPT
/
RWPT
/
RGFT
/
RWFT
/
ROIP
/
ROP
/
ROPR
/
RGPR
/
RWPR
/
RGIR
/
RGIT
/
RWIR
/
RWIT
/
RWPT
/
ROIPL
/
ROIPG
/
RGIP
/
RGIPL
/
RGIPG
/
RWIP
/
RPPO
/

--  Group data --
GPR
/
GLPR
/
GOPT
/
GGPT
/
GWPT
/
GNPT
/
GOPR
/
GGPR
/
GWPR
/
GWPRH
/
GGIR
/
GNPR
/

GNIR
/
GGIRH
/
GGIT
/
GNIT
/
GGITH
/
GWCT
/
GWCTH
/
GGOR
/
GGORH
/
GWIR
/
GWIT
/
GWIRH
/
GWITH
/
GOPRH
/
GGPRH
/
GLPRH
/
GWPTH
/
GOPTH
/
GGPTH
/
GLPTH
/
GPRG
/
GPRW
/
GOPTF
/
GOPTS
/
GOPTH
/
GOPRF
/
GOPRS
/
GOPRH
/
GGPTF
/
GGPTS
/
GGPTH
/
GGPTF
/
GGPTS
/
GGPTH
/
GGLR
/
GGLIR
/
GGLRH
/
GVPR
/
GVPT
/
GMCTP
/
GOPP
/
GVIR
/
GVIT
/
GVPRT
/
GMWPR
/
GMWIN
/

GVPR
/

GVPT
/
-- Well Data
-- Production Rates
WWPR
/
WWPRH
/
WOPR
/
WOPRH
/
WGPR
/
WNPR
/
WGPRH
/
WLPR
/
WLPRH
/

WLPT
/

WLPTH
/

WCPR
/

-- Production Cummulatives
WWPT
/
WWPTH
/
WOPT
/
WOPTH
/
WGPT
/
WGPTH
/
WNPT
/

WCPT
/

-- Tracers
--WTPRSEA
--/
--WTPTSEA
--/
-- Injection Cummulatives
-- Ratios
WWCT
/
WWCTH
/
WGOR
/
WGORH
/
WGLR
/
WGLRH
/


-- Performance
WBHP
/
WBHPH
/
WTHP
/
WTHPH
/
WPI
/
WBP
/
WBP4
/

-- from model2
WOPTF
/
WOPTS
/
WOPTH
/
WOPRS
/
WOPRF
/
WGPTF
/
WGPTS
/
WGPRF
/
WTPRS
/
WGLIR
/
WVPR
/
WVPT
/
WOPP
/
WVIR
/
WVIT
/
WMCTL
/

-- Water injection per connection
CWIR
  * /
/


CGIT
* /
/

-- Production per connection
-- Using all the different ways of specifying connections here
-- as an informal test that we still get the data we want
CWPR
 'W_1' 1 1 1 /
/

COPR
 'W_1' /
 'W_2' /
/

CGPR
 '*' /
/

CNFR
 '*' /
/

CNPT
 '*' /
/

CNIT
 '*' /
/

CWPT
 'W_1' 1 1 1 /
/

COPT
 'W_1' /
/

CGPT
 'W_1' /
 'W_2' /
/

---- Connection production rates
----CGFR
----'E-4AH' /
----/
----CWFR
----'E-2H' /
----/

SCHEDULE

GRUPTREE
  'G_1'  'G' /
  'G_2'  'G' /
/


WELSPECS
     'W_1'        'G_1'   1    1  3.33       'OIL'  7* /
     'W_2'        'G_2'   2    1  3.33       'OIL'  7* /
/

-- Completion data.
COMPDAT
-- 'Well' I J K1 K2
-- Passing 0 to I/J means they'll get the well head I/J
    W_1 0 0 1 1 /   -- Active index: 0
    W_2 0 0 1 1 /   -- Active index: 1
    W_2 0 0 2 2 /   -- Active index: 101
/

WCONHIST
-- history rates are set so that W_1 produces 1, W_2 produces 2 etc.
-- index.offset.
-- organised as oil-water-gas
    W_1 'OPEN' ORAT 10.1 10 10.2 /
    W_2 'OPEN' ORAT 20.1 20 20.2 /
/


TSTEP
-- register time steps (in days). This allows us to write *two* report steps (1
-- and 2. Without this, totals/accumulations would fail (segfault) when looking
-- up historical rates and volumes. These volumes however don't change, i.e.
-- every time step has the same set of values
10 10 /


TSTEP
10 10 /
