{"name" : "EQUIL" , "sections" : ["SOLUTION"], "size" : {"keyword":"EQLDIMS" , "item":"NTEQUL"},
 "description": "The EQUIL item is used when equilibrationg the model. The item should consist of one record for each PVT region",
 "items" :
 [{"name" : "DATUM_DEPTH"       , "value_type" : "DOUBLE" , "default" : 0.0 , "dimension" : "Length"},
  {"name" : "DATUM_PRESSURE"    , "value_type" : "DOUBLE" , "dimension" : "Pressure"} ,
  {"name" : "OWC"               , "value_type" : "DOUBLE" , "default" : 0.0 , "dimension" : "Length",
            "description" : "The OWC item is depth of the OIL Water contact. This should ..."} ,
  {"name" : "PC_OWC"            , "value_type" : "DOUBLE" , "default" : 0.0 , "dimension" : "Pressure"} ,
  {"name" : "GOC"               , "value_type" : "DOUBLE" , "default" : 0.0 , "dimension" : "Length"} ,
  {"name" : "PC_GOC"            , "value_type" : "DOUBLE" , "default" : 0.0 , "dimension" : "Pressure"} ,
  {"name" : "BLACK_OIL_INIT"    , "value_type" : "INT" , "default" : 0} ,
  {"name" : "BLACK_OIL_INIT_WG" , "value_type" : "INT" , "default" : 0} ,
  {"name" : "OIP_INIT"          , "value_type" : "INT" , "default" : -5 , "comment":"The default is a state variable"}]}
